Source: /media/dave/0DD7-140D/Projects/Monster Schematics/MPU & ACIA/MPU & ACIA.kicad_sch
Date: Mon 11 Sep 2023 04:15:02 PM PDT
Tool: Eeschema 6.0.2+dfsg-1
Generator: /usr/share/kicad/plugins/bom_csv_grouped_by_value_with_fp.py
Component Count: 20

Ref 	Qnty 	Value 	Cmp name 	Footprint 	Description Vendor
C1,  	1 	10uF 	C_Polarized_US  Polarized capacitor, US symbol 
C2, C3, 2 	22pF 	C  Unpolarized capacitor 
C4-6,  	3 	0.1uF 	C  Unpolarized capacitor 
D1,  	1 	LED (Green) LED  Light emitting diode 
J1,  	1 	1x40-Backplane/Busses Conn_01x40_MountingPin, single row, 01x40
J2,  	1 	1x03_Male Conn_01x03_Male  Generic connector, single row, 01x03
R1-2, R4, 3 	4.7K 	R_US  Resistor, US symbol 
R3,  	1 	220-330 R_US  Resistor, US symbol 
SW1,  	1 	Momentary SW_MEC_5G  MEC 5G single pole normally-open tactile switch 
SW2,  	1 	SW_DIP_x04 SW_DIP_x04  4x DIP Switch, Single Pole Single Throw (SPST)
U1,  	1 	MC6802 	DIP-40_W15.24mm 8-Bit Microprocessing unit 1.0MHz, DIP-40 
U2,  	1 	74LS393 Dual BCD 4-bit counter 
U3,  	1 	MC6850 	Package_DIP:DIP-24_W15.24mm Asynchronous Communications Interface Adapter 1MHz
X1,  	1 	4.9152 MHz XO32 Oscillator:Oscillator_SMD_EuroQuartz_XO32-4Pin_3.2x2.5mm HCMOS Clock Oscillator 
Y1,  	1 	4 MHz Crystal  Two pin crystal 



Source: /media/dave/0DD7-140D/Projects/Monster Schematics/RAM and ROM.kicad_sch
Component Count: 17

Ref 	Qnty 	Value 	Cmp name 	Footprint 	Description Vendor
C1, C2, C3, C5, C7,  5 0.1uF C  Unpolarized capacitor 
C4,  1 100uF C_Polarized_US  Polarized capacitor, US symbol 
C6,  1 10uF C_Polarized_US  Polarized capacitor, US symbol 
J1,  1 Conn_01x40-Backplane/Busses Conn_01x40_MountingPin  Generic connectable mounting pin connector, single row, 01x40, script generated (kicad-library-utils/schlib/autogen/connector/) 
J2,  1 DC 5-9V Barrel_Jack_Switch  DC Barrel Jack with an internal switch 
R1,  1 4.7K R_US  Resistor, US symbol 
SW1,  1 SW_SPST SW_SPST  Single Pole Single Throw (SPST) switch 
U1,  1 74LS00 74LS00  quad 2-input NAND gate 
U2,  1 74LS04 74LS04  Hex Inverter 
U3,  1 74LS138 74LS138  Decoder 3 to 8 active low outputs 
U4,  1 28C256 28C256  Paged Parallel EEPROM 256Kb (32K x 8), DIP-28/SOIC-28 
U5,  1 L7805 L7805  Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252 
U6,  1 CY62256-70PC CY62256-70PC Package_DIP:DIP-28_W15.24mm 256K (32K x 8) Static RAM, 70ns, DIP-28 


TOTAL
=====
Capacitors:
22pF		2
0.1uF		8
10uF (elec)	2
100uF (elec)	1

Diodes:
LED (Green)	1

Connectors:
1x40 M (rt ang)	2
1x03_Male Conn	1
DC Barrel_Jack	1

Resistors:
4.7K		4
220-330		1

Switches:
Momentary SPST	1	[6.5 x 5 mm]
4x DIP SPST	1
Toggle SPST	1	[rt. angle]

ICs:
6802		1
6850		1
74LS393		1
74LS00		1
74LS04		1
74LS138		1
28C256		1
L7805		1
62256		1

Crystals:
4.9152 MHz Osc	1
4 MHz two pin	1
1.8432MHz 2-pin 1

Sockets:
40-pin		1
28-pin		1
24-pin		1
14-pin (N)	3
16-pin (N)	1
4-pin (1/2 osc)	1
28-pin ZIF	1

